ShapeCorrect 4.00
ShapeCorrect Output: 
   Corrected and uncorrected GPS positions.
 
ShapeCorrect results for layer Z:\gis564\lab4\QuickProject 2008-05-20 1341\Lines.shp
Creating Z:\gis564\lab4\QuickProject 2008-05-20 1341\Lines.bkp as a backup copy of the original shapefile
Error: The number of positions in the SSF and COR files are different.
This is probably because Differential Correction is configured to output 'Corrected Only'.
It must be configured to output 'Corrected and Uncorrected' in the Output tab of the GPS Settings dialog.
 
ShapeCorrect results for layer Z:\gis564\lab4\QuickProject 2008-05-20 1341\Points.shp
Creating Z:\gis564\lab4\QuickProject 2008-05-20 1341\Points.bkp as a backup copy of the original shapefile
Error: The number of positions in the SSF and COR files are different.
This is probably because Differential Correction is configured to output 'Corrected Only'.
It must be configured to output 'Corrected and Uncorrected' in the Output tab of the GPS Settings dialog.
 
ShapeCorrect results for layer Z:\gis564\lab4\QuickProject 2008-05-20 1341\Polygons.shp
Creating Z:\gis564\lab4\QuickProject 2008-05-20 1341\Polygons.bkp as a backup copy of the original shapefile
Error: The number of positions in the SSF and COR files are different.
This is probably because Differential Correction is configured to output 'Corrected Only'.
It must be configured to output 'Corrected and Uncorrected' in the Output tab of the GPS Settings dialog.
